# Instructions for Installing the Software Update

1. Copy the .kf1 software update package to the root directory of a USB drive
   formatted in FAT32

2. Insert the USB drive in a Diva LUX 4, Celeb IKON 6, or Celeb IKON 12 light
   fixture

3. If the fixture has been running for more than a few minutes, disconnect and
   reconnect power to the fixture before continuing.

4. On the fixture's screen, select [Admin], then [Mntn], then [Save]

5. Wait a moment for the fixture's settings to save to the USB drive,
   then select [Update] to install the software

6. Wait for the update to complete and for the fixture to reboot. Do not touch
   the USB drive during this process.

7. Optional — to update the fixture's default IP address to be Art-Net 4
   compliant, select [Admin], then [Mntn], then [Factory Reset]


If you have any issues please contact Chauvet Cinema support by email:
Info@ChauvetCinema.com; or phone: +1 (818) 358-8542
